

**Specially Prepared For**

**John Doe**

321 Elm St.

Wenatchee, WA 98801

*Prepared by*

**Contractor Name**

email@website.com

(555) 555-5555

Month XX, Year

# CONTRACTOR STATEMENT

The following project measures have been designed and formulated specifically for your home. **Contractor Name** is committed to finding the best ways to make your home more energy efficient and comfortable.

**WHOLE HOME AIR SEALING**

**$X,XXX**

* Perform Blower Door Guided air sealing.
* Seal accessible plumbing and electrical penetrations between conditioned and unconditioned spaces.
* Prioritize sealing connections to the attic and crawlspace/basement for better interior air quality and moisture control.
* Air sealing measure will be completed to local utility Air Sealing specifications.

**Available rebates: $XX.XX** (not deducted from price shown)

**DUCT SEALING AND INSULATION**

**$X,XXX**

* All accessible portions of the duct system shall be repaired, mechanically fastened and sealed where applicable.
* Insulate ductwork with **R-19 formaldehyde-free fiberglass** insulation with vinyl backing.
* All accessible connections to be inspected and repaired to local utility specifications.

**Available rebates: Up to $XX.XX** (not deducted from price shown)

**FLOOR INSULATION**

**$X,XXX**

* Install 839 sq. ft. of **R-19 formaldehyde-free fiberglass** insulation batts in crawlspace ceiling and twine in place for continuous contact to heated floor for increase comfort.
* **Final R-value to be R-30.**
* Insulate and weatherstrip crawlspace hatch.
* Install 6-mil polyethylene ground barrier on crawlspace floor to reduce moisture and particle intrusion.
* Install (1) new foundation vent for proper ventilation per code.
* Drill and Fill 133 sq. ft. of cantilever with **fiberglass blown to R-25**.
* All items to be installed to BPA and local utility specifications.
* Plumbing and ducts to be inspected for leaks and disrepair. Any newly found problems will be communicated to homeowner and an estimate may be provided to undertake corrective work.

**Available rebates: $XX.XX** (not deducted from price shown)

**ATTIC INSULATION**

**$X,XXX**

* Remove existing insulation and dispose/recycle debris.
* Dam around attic hatch with ½” plywood, weatherstrip and insulate hatch with **rigid foam board insulation** to **R-30**.
* Install baffles at existing lower eave vents.
* Baffle around existing bath fan. Install insulated hard duct and connect to new dedicated exterior termination with damper.
* Install (1) new metal 8” RV50 roof vent per code.
* Install 839 sq. ft. of blown-in **formaldehyde-free fiberglass** insulation to **R-49**.

**Available rebates: $XX.XX** (not deducted from price shown)

**WALL INSULATION**

**$X,XXX**

**1st Floor**

* Remove siding as necessary for wall insulation installation on 1st floor.
* Install 1355 sq. ft of dense packed **formaldehyde-free fiberglass** insulation to **R-15** in 1st floor walls.
* Weather seal, and reinstall original siding. Repair walls with new plugs and texture to blend as close as possible with existing texture.
* No painting included.

**2nd Floor**

* Install dust protection as necessary for interior wall insulation installation in 2nd floor walls.
* Install 738 sq. ft. of dense packed **formaldehyde-free fiberglass** insulation to **R-15** in 2nd floor walls.
* Repair walls with new plugs and texture to blend as close as possible with existing texture.
* No painting included.

**Available rebates: $XX.XX** (not deducted from price shown)

**BRAND AIR SOURCE HEAT PUMP**

**$X,XXX**

* Remove and properly dispose/recycle existing heat pump air handler, outside unit, and refrigerant lines.
* Furnish and install the new 3 ton XP25 modulating compressor heat pump with air handler and variable speed fan motor.
* 10 HSPF/ 22 SEER efficiency
* Fabricate and install sheet metal fittings to accommodate furnace.
* Furnish and install new PVC venting and combustion air intake to exterior.
* Furnish and install condensate pump.
* Start up, test, and adjust equipment to PTCS and local utility specifications and requirement for optimal efficiency.
* Required HVAC permit included.
* 10-year limited warranty
* Also Included: Provide and install MERV 12 air purification system at time of install.

**Available rebates: $XX.XX** (not deducted from price shown)

**BRAND HEAT PUMP WATER HEATER**

**$X,XXX**

* Drain, remove and dispose/recycle existing hot water heater.
* Install new rebate qualifying 50-gallon Brand Heat Pump Water Heater.
* Install needed duct to exterior, drain line, seismic strapping, drain pan and T&P valve.
* Connect water heater to existing electrical.
* Install new plumbing connections and connect to existing water lines.
* Permit included.
* Water Heater to be installed to manufacturer and local utility specifications.
* **10-year** limited warranty.

**Available rebates: $XX.XX** (not deducted from price shown)

Total Investment Price:

$X,XXX

Utility Rebates and Incentives:

$X,XXX

Available Tax Credit:

$X,XXX

**Total Price:**

**$X,XXX or $XX.XX/month**

**I accept this proposal**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Homeowner**

**Project Also Includes:** Preparation of your home for dust protection and safety | Careful removal of existing attic and floor insulation | Disposal/recycling fees | Lead Testing (if Lead is found a change order for proper removal may be required) | Delivery of materials | Professional installation by Contractor Name’s trained installers | 3-year installation warranty

**Rebates, Incentives and Tax Credits:** Rebates are estimated based on your local utility’s offerings. Incentives and tax credits are estimates and are not guaranteed based on your personal tax liability.



**Contractor Name**

123 Main St.

Wenatchee, WA 98801

(555) 555-5555